There are two codes posted here, the first is in response to the IR emitter, the second in response to the hand-held remote

Emitter input